|  |  |
| --- | --- |
| FEDERATION  INTERNATIONALE  DE L'AUTOMOBILE  WWW.FIA.COM | **APPLICATION FOR THE APPROVAL OF THE TECHNICAL REGULATIONS**  **OF AN INTERNATIONAL SERIES BY THE FIA**  **IN ACCORDANCE WITH ART. 2.4 OF THE INTERNATIONAL SPORTING CODE** |

**Reminder**

**In order to be eligible for an FIA International Series, the Technical Regulations must include and respect the safety requirements in conformity with Appendix J, and in particular with regard to the following points:**

* Total conformity with one of the Groups defined in Appendix J.
  + Total conformity with Article 277 of Appendix J (minimum safety requirements).

Not applicable when the car is homologated by the FIA or is in conformity with another FIA Group.

* + In the event that total conformity with Appendix J is not possible, the application for the approval of the series must explicitly mention the elements that do not respect Appendix J.

Any element indicated "NO" in the following tables must be the subject of an explanatory document to be appended to the present form.

According to the information received, the FIA Administration, after consultation with the requesting ASN, will decide whether or not partial conformity is acceptable for safety reasons and will make a recommendation to the World Council to accept or reject the international series.

🞿🞿🞿🞿

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | | | | |
| The | | | **\*SPECIFY ASN NAME\*** | | | | | On | | **\*SPECIFY DATE OF APPLICATION\*** | | |  |
|  | | | | | | | | | | | | | |
| hereby declares that the vehicles to be entered in the International Series designated : | | | | | | | | | | | | |  |
|  | | | | | | | | | | | | | |
|  | | | **\*SPECIFY SERIES NAME\*** | | | | | For | | **\*SPECIFY YEAR/SEASON\*** | | |  |
|  | | | | | | | | | | | | | |
| fulfils the eligibility criteria mentioned above and are as per the descriptions below. | | | | | | | | | | | | |  |
|  | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
| **A.** | **VEHICLES IN COMPLIANCE WITH GROUPS OF APPENDIX J** | | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | | | | | **ARTICLES OF APPENDIX J**  (EXCEPT ART. 251, 252, 253, 277, 281, 282, 283) | | | | | | |  |
|  | | | | | | | | | | | | | |
|  | **\*SPECIFY CATEGORY'S NAME\*** | | | ⮊ | | **"SPECIFY ARTICLE CONCERNED, E.G. 257A"** | | | | | | |  |
|  | | | | | | | | | | | | | |
|  |  | | | ⮊ | |  | | | | | | |  |
|  | | | | | | | | | | | | | |
|  |  | | | ⮊ | |  | | | | | | |  |
|  | | | | | | | | | | | | | |
|  |  | | | ⮊ | |  | | | | | | |  |
|  | | | | | | | | | | | | | |
|  |  | | | ⮊ | |  | | | | | | |  |
|  | | | | | | | | | | | | | |
|  |  | | | ⮊ | |  | | | | | | |  |
|  | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
| B. | | **VEHICLES IN COMPLIANCE WITH ART. 277 OF APPENDIX J** *Other than those defined in one of the groups of Appendix J* | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
|  | | **CATEGORY\***  *\*as specified in the technical regulations of the series* | | | | | **CATEGORY OF ART. 277\***  *\*can only be I, II-SH, II-SC, II-SS, III* | | | | | |  |
|  | | | | | | | | | | | | | |
|  | | **\*SPECIFY CATEGORY'S NAME\*** | | | ⮊ | | **\*E.G. II-SC\*** | | *see table n°* | | **\*E.G. B2-1\*** | *below* |  |
|  | | | | | | | | | | | | | |
|  | |  | | | ⮊ | |  | | *see table n°* | |  | *below* |  |
|  | | | | | | | | | | | | | |
|  | |  | | | ⮊ | |  | | *see table n°* | |  | *below* |  |
|  | | | | | | | | | | | | | |
|  | |  | | | ⮊ | |  | | *see table n°* | |  | *below* |  |
|  | | | | | | | | | | | | | |
|  | |  | | | ⮊ | |  | | *see table n°* | |  | *below* |  |
|  | | | | | | | | | | | | | |
|  | |  | | | ⮊ | |  | | *see table n°* | |  | *below* |  |
|  | | | | | | | | | | | | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B1.1** | **CHECK LIST TABLE FOR VEHICLES COMPARABLE TO CATEGORY I (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | Safety tank | FT3, FT3.5 or FT5 specification compulsory, in compliance with the prescriptions of Art. 253-14 | |  |  |  |
|  | Fuel pipes, pumps and filters | 253-3.1 and 253-3.2 | |  |  |  |
|  | Tank fillers and caps | 259-6.4 | |  |  |  |
|  | Refuelling during the race (circuit) | 277-2.3 | |  |  |  |
|  | Fuel | 252-9 | |  |  |  |
|  | Oil catch tank | 255-5.1.14 of the 2019 Appendix J | |  |  |  |
|  | Safety belts | 253-6 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 and 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 253-7 | |  |  |  |
|  | Rear-view mirrors | 253-9 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Towing eye | 253-10 | |  |  |  |
|  | Firewall | 253-15 | |  |  |  |
|  | Seats | 253-16 | |  |  |  |
|  | Windscreen | 279-10.2.2 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 252-2.1 | |  |  |  |
|  | Battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 253-8 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 253-8 | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B1.2** | **CHECK LIST TABLE FOR CROSS-COUNTRY-TYPE VEHICLES COMPARABLE TO CATEGORY I (ART. 281-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 283-4 | |  |  |  |
|  | Circuit breaker | 283-13 | |  |  |  |
|  | Safety tank | FT3, FT3.5 or FT5 specification compulsory, in compliance with the prescriptions of Art. 283-14 | |  |  |  |
|  | Fuel pipes, pumps and filters | 283-3.1 et 283-3.2 | |  |  |  |
|  | Tank fillers and caps | 283-14.2 et 283-14.3 | |  |  |  |
|  | Fuel | 282-9 | |  |  |  |
|  | Safety belts | 283-6 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 282-5 | |  |  |  |
|  | Wheel material | 282-6 | |  |  |  |
|  | Extinguishers | 283-7 | |  |  |  |
|  | Rear-view mirrors | 283-9 | |  |  |  |
|  | Lighting equipment | 283-16 | |  |  |  |
|  | Towing eye | 283-10 | |  |  |  |
|  | Firewall | 283-15 | |  |  |  |
|  | Seats | 283-20 | |  |  |  |
|  | Windscreen | 283-11 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 282-2.1 | |  |  |  |
|  | Battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks. | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 283-8 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 283-8 | |  |  |  |
|  | Minimum weight | 277-3 and 284-5 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B1.3** | **CHECK LIST TABLE FOR ELECTRICALLY-POWERED VEHICLES COMPARABLE TO CATEGORY I (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Crash test | Must satisfy the FIA guidelines for crash test (available upon request from the FIA Technical Department) | |  |  |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | High Voltage system | 253-18 | |  |  |  |
|  |  | All High Voltage systems must be Original Equipment Manufacturer (OEM) (those of the series production car homologated for road use), with the exception of modifications made by the car manufacturer | |  |  |  |
|  |  | FIA approval compulsory for International Series approved by the FIA | |  |  |  |
|  | Safety belts | 253-6 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 and 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 253-7 and 253-18.23 | |  |  |  |
|  | Rear-view mirrors | 253-9 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Towing eye | 253-10 | |  |  |  |
|  | Firewall | 253-15 | |  |  |  |
|  | Seats and seat mountings | 253-16 | |  |  |  |
|  |  | ASN Homologation or Certification compulsory for International Series approved by the FIA | |  |  |  |
|  | Windscreen | 279-10.2.2 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 252-2.1 | |  |  |  |
|  | Auxiliary battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks | |  |  |  |
|  | Safety structures | The safety cage must be Homologated or Certified by an ASN according to the FIA homologation regulations for safety cages (see Article 253-8.1) | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.1** | **CHECK LIST TABLE FOR VEHICLES COMPARABLE TO CATEGORY II-SH (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | Safety tank – General case | 259-6.3 | |  |  |  |
|  | Safety tank – GT-type cars | 257A-6.3 of Appendix J 2015 for tank | |  |  |  |
|  |  | 253-3.4 for ventilation | |  |  |  |
|  | Compulsory automatic fuel cut-off  **GT-type cars only** | 253-3.3 | |  |  |  |
|  | Fuel pipes, pumps and filters | 253-3.1 and 253-3.2 | |  |  |  |
|  | Tank fillers and caps | 259-6.4 | |  |  |  |
|  | Refuelling during the race (circuit) | 277-2.3 | |  |  |  |
|  | Fuel | 252-9 | |  |  |  |
|  | Oil catch tank | 259-7.4 | |  |  |  |
|  | Safety belts | 259-14.2.1 | |  |  |  |
|  | Longitudinal location of the oil system  (except for rear-engine vehicles) | 275-7.2 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 and 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 253-7 | |  |  |  |
|  | Rear-view mirrors | 253-9 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Towing eye | 259-14.6 | |  |  |  |
|  | Firewall | 259-16.6 | |  |  |  |
|  | Seats | 253-16 | |  |  |  |
|  | Windscreen | 279-10.2.2 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 252-2.1 | |  |  |  |
|  | Battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 253-8 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 253-8 | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.2** | **CHECK LIST TABLE FOR ELECTRICALLY-POWERED VEHICLES**  **COMPARABLE TO CATEGORY II-SH (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Crash test | Must satisfy the FIA guidelines for crash test (available upon request from the FIA Technical Department) | |  |  |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | High Voltage system | 253-18 | |  |  |  |
|  |  | All High Voltage systems must be Original Equipment Manufacturer (OEM) (those of the series production car homologated for road use), with the exception of modifications made by the car manufacturer | |  |  |  |
|  |  | FIA approval compulsory for International Series approved by the FIA | |  |  |  |
|  | Safety belts | 259-14.2.1 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 et 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 283-7 and 253-18.23 | |  |  |  |
|  | Rear-view mirrors | 253-9 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Towing eye | 259-14.6 | |  |  |  |
|  | Firewall | 259-16.6 | |  |  |  |
|  | Seats and seat mountings | 253-16 | |  |  |  |
|  | Windscreen | 279-10.2.2 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 252-2.1 | |  |  |  |
|  | Auxiliary battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks | |  |  |  |
|  | Safety structures | The safety cage must be Homologated or Certified by an ASN according to the FIA homologation regulations for safety cages (see Article 253-8.1) | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.3** | **CHECK LIST TABLE FOR CROSS-COUNTRY-TYPE VEHICLES COMPARABLE TO CATEGORY II (ART. 281-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 283-4 | |  |  |  |
|  | Circuit breaker | 283-13 | |  |  |  |
|  | Safety tank | FT3, FT3.5 or FT5 specification compulsory, in compliance with the prescriptions of Art. 283-14 | |  |  |  |
|  | Fuel pipes, pumps and filters | 283-3.1 et 283-3.2 | |  |  |  |
|  | Tank fillers and caps | 283-14.2 et 283-14.3 | |  |  |  |
|  | Fuel | 282-9 | |  |  |  |
|  | Oil catch tank | 285-5.2 | |  |  |  |
|  | Safety belts | 283-6 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 282-5 | |  |  |  |
|  | Wheel material | 282-6 | |  |  |  |
|  | Extinguishers | 283-7 | |  |  |  |
|  | Rear-view mirrors | 283-9 | |  |  |  |
|  | Rear light | 283-16 | |  |  |  |
|  | Towing eye | 283-10 | |  |  |  |
|  | Firewall | 283-15 | |  |  |  |
|  | Seats | 283-20 | |  |  |  |
|  | Windscreen | 285-3.1 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 282-2.1 | |  |  |  |
|  | Battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks. | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 283-8 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 283-8 | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.4** | **CHECK LIST TABLE FOR CROSS-COUNTRY-TYPE ELECTRICALLY-POWERED VEHICLES**  **COMPARABLE TO CATEGORY II (ART. 281-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Crash test | Must satisfy the FIA guidelines for crash test (available upon request from the FIA Technical Department) | |  |  |  |
|  | Brake system safety | 283-4 | |  |  |  |
|  | Circuit breaker | 283-13 | |  |  |  |
|  | High Voltage system | 283-18 | |  |  |  |
|  |  | All High Voltage systems must be Original Equipment Manufacturer (OEM) (those of the series production car homologated for road use), with the exception of modifications made by the car manufacturer | |  |  |  |
|  |  | FIA approval compulsory for International Series approved by the FIA | |  |  |  |
|  | Safety belts | 283-6 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 282-5 | |  |  |  |
|  | Wheel material | 282-6 | |  |  |  |
|  | Extinguishers | 283-7 and 253-18.23 | |  |  |  |
|  | Rear-view mirrors | 283-9 | |  |  |  |
|  | Rear light | 283-16 | |  |  |  |
|  | Towing eye | 283-10 | |  |  |  |
|  | Firewall | 283-15 | |  |  |  |
|  | Seats | 283-20 | |  |  |  |
|  | Windscreen | 285-3.1 | |  |  |  |
|  | Ground clearance | 282-2.1 | |  |  |  |
|  | Auxiliary battery(ies) | Each battery must be securely fixed and covered to avoid any short-circuiting or leaks. | |  |  |  |
|  | Safety structures | The safety cage must be Homologated or Certified by an ASN according to the FIA homologation regulations for safety cages (see Article 283-8.1) | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.5** | **CHECK LIST TABLE FOR VEHICLES COMPARABLE TO CATEGORY II-SC (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | Safety tank – General case | 259-6.3 | |  |  |  |
|  | Fuel pipes, pumps and filters | 253-3.1 and 259-6.2 | |  |  |  |
|  | Tank fillers and caps | 259-6.4 | |  |  |  |
|  | Refuelling during the race (circuit) | 277-2.3 | |  |  |  |
|  | Fuel | 252-9 | |  |  |  |
|  | Oil catch tank | 259-7.4 | |  |  |  |
|  | Safety belts | 259-14.2.1 | |  |  |  |
|  | Longitudinal location of the oil system  (except for rear-engined vehicles) | 275-7.2 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 and 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 275-14.1 | |  |  |  |
|  | Rear-view mirrors | 275-14.3.1+14.3.2+14.3.4 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Headrest | 259-14.4 | |  |  |  |
|  | Towing eye | 259-14.6 | |  |  |  |
|  | Firewall | 259-16.6 | |  |  |  |
|  | Windscreen | 259-3.6 | |  |  |  |
|  |  | A windscreen wiper in working order is mandatory | |  |  |  |
|  |  | An efficient windscreen demisting system is mandatory | |  |  |  |
|  | Ground clearance | 252-2.1 | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 259-15.1 (vehicles built **before** 01.01.2004)  259-16.4 (vehicles built **as from** 01.01.2004)  283-8 (Cross-country vehicles) | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 259-16.4  283-8 (Cross-country vehicles) | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B2.4** | **CHECK LIST TABLE FOR VEHICLES COMPARABLE TO CATEGORY II-SS** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 275-11.1 | |  |  |  |
|  | Master switch | 275-14.2 | |  |  |  |
|  | Safety tank | 259-6.3  275-6.1 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Fuel pipes, pumps and filters | 259-6.2 | |  |  |  |
|  | Tank fillers and caps | 259-6.4 | |  |  |  |
|  | Refuelling during the race (circuit) | 277-2.3 | |  |  |  |
|  | Fuel | 252-9 | |  |  |  |
|  | Oil catch tank | 259-7.4 | |  |  |  |
|  | Safety belts | 275-14.4 | |  |  |  |
|  | Longitudinal location of the oil system | 275-7.2 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 et 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Cockpit opening | 275-13.1 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Extinguishing system | 275-14.1 | |  |  |  |
|  | Rear-view mirrors | 275-14.3 | |  |  |  |
|  | Rear light | 275-14.5 | |  |  |  |
|  | Headrest | 275-14.6 | |  |  |  |
|  | Seat fixing and removal | 275-14.7 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Steering column | 275-10.10.3 and 275-10.10.4 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Suspension anti intrusion bars | 277-2.2.1.1 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Pedal position | 275-13.4 (vehicles built as from 01.01.2010) | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 277-2.1 and 277-2.1.1 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 277-2.2.1 | |  |  |  |
|  | Minimum weight | 277-3 | |  |  |  |
|  | Bodywork / Cockpit | 277-4 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **B3** | **CHECK LIST TABLE FOR VEHICLES COMPARABLE TO CATEGORY III (ART. 251-1.1)** | | | | | |
|  | | | | | | |
|  | **CATEGORY\***  *\*as specified in the technical regulations of the series* | |  | | |  |
|  | | | | | | |
|  | **Safety item/device** | **Article of Appendix J** | | **Compliance** | |  |
|  | **YES** | **NO** |  |
|  | Brake system safety | 253-4 | |  |  |  |
|  | Circuit breaker | 253-13 | |  |  |  |
|  | Safety tank | 259-6.3 | |  |  |  |
|  | Fuel pipes, pumps and filters | 259-6.2 | |  |  |  |
|  | Tank fillers and caps | 259-6.4 | |  |  |  |
|  | Refuelling during the race (circuit) | 277-2.3 | |  |  |  |
|  | Fuel | 252-9 | |  |  |  |
|  | Oil catch tank | 259-7.4 | |  |  |  |
|  | Safety belts | 259-14.2.1 | |  |  |  |
|  | Longitudinal location of the oil system | 275-7.2 | |  |  |  |
|  | Reverse gear | 275-9.4 | |  |  |  |
|  | Suspension arm | 275-10.3 and 275-10.4.1 | |  |  |  |
|  | Wheel material | 275-12.2 | |  |  |  |
|  | Extinguishers | 290.2.7 | |  |  |  |
|  | Rear-view mirrors | 290.2.13 | |  |  |  |
|  | Rear light | 259-8.4.2 | |  |  |  |
|  | Towing eye | 259-14.6 | |  |  |  |
|  | Firewall | 259-16.6 | |  |  |  |
|  | Seats | 253-16 | |  |  |  |
|  | Safety structures of vehicles built  **before** 01.01.2010 | 259-16.4 | |  |  |  |
|  | Safety structures of vehicles built  **as from** 01.01.2010 | 287-3.1 or 290-2.9 | |  |  |  |
|  | Aerodynamic devices | 277-5 | |  |  |  |
|  | | | | | | |

**NB :** This page may be duplicated if there is more than one category of vehicles concerned